MARATHON.txt 6.3          APRS at the Marine Corps Marathon 1993 (and 4)

APRS LESSONS LEARNED @ MC Marathon, 1994!
Its over!  14,000 runners, LOTS of hams, and our second year with APRS!  Last
year we had GPS on the LEAD, LEAD Handicapped, & TAIL chase cars. It was great,
but predictible.  This year we let APRS dead-reckon the predictible movements
of the chase cars and built 11 Trackers for the ambulances.  Lessons learned:
 * Completely "sealed" GPS/TNC/Radio boxes should have drain holes in bottom!
 * Maritime GPS units withstand immersion in water. TNC's don't
 * You can't duct-tape GPS trackers to vehicles in the pouring rain
 * New Marine Corps Tents (made by lowest bidder) leaked everywhere!
 * 14,000 runners, vehicles, etc + RAIN = MUD
 * Mag-mount GPS trackers wont stick to aluminum HUM-VEES.
 * Tracking ambulances, which are parked for 99% of the event is BORING!
 * Ambulances with emergencies are under such close control by the ambulance
   direction net control, that he knows EXACTLY where they are anyway.
Of 11 units, 2 never quite got finished, one just couldn't be attached in the
rain, one leaked, flooded and died, the tinyest (running on AA cells) lasted
6 hours.  It rained from 5 AM until 1400.  Now for the good news:
 + We got double milage out of most APRS mobiles.  They put their GPS's in
   stand alone trackers for the ambulances, but kept their LAPTOPS and used
   the INPUT-MY command to manually report their position.
 + The alt-IGNORE command let the entire event operate on 145.79 while
   ignoring ALL other non-participating stations.  THis keeps all APRS pages
   free of non-participants.  But the transitioning in an out of
   this SPCL mode needs some more work.  Many stand-alone trackers are XTAL
   controlled, so you MUST plan on using the normal APRS freq for spcl events.

CONCLUSIONS:  Next year, we will probably go back to tracking the high-profile
chase vehicles and HAM mobiles that are always moving, rather than ambulances.
These 11 trackers now are permanent HAM radio assets in our community in
addition to the other 6 HAM mobiles that are permanently configured for APRS.


SUMMARY OF 1993 MARATHON!

     The complete event can be re-played from MARATHON.hst to see how it
went.  To make sense out of it all, play back only one mobile at a time, and
turn Callsigns off.  WB4APR-9 was the lead Handicapped vehicle (started 15
minutes or so before all runners), W3ADO-9 was the lead runner, and MOBILE-9
was Tail-end-Charlie.  Statistically, we did very well.  W3ADO-9 was turned on
at 0827 but did not move until 0902.  It was removed from the vehicle at about
1127.  Transmitting at once a minute, there should have been 145 posits trans-
mitted.  We counted about 115 in the file.  The missing packets could have been
either colisions, or bad GPS fixes (masked by buildings) so that the same posit
was transmitted more than once (and therefore filtered out as a dupe by APRS).
The result computes to almost an 80% success rate!

