NEWNOTES.TXT     * * * *  NEW STUFF ADDED IN EACH NEW VERSION  * * * *

Ver 72: Meteor Scatter mode!  EVERYONE is needed to participate!
* New METEOR SHOWER mode for upcoming Persieds 11 to 15 Aug.  See METEOR.txt
* SPACE mode resets BEACON timer on hearing space digipeater. See Space.txt
* If CONTROLS-FILTERS-GdSq is on, APRS will use gridsq's in the TO address
* Hopefully fixed the cmd: showing up in packets
* Rain should now zero when you reset your U-II rain counters
* Better map border display colors and ranges.
* KB8JXO, the ultimate map maker, made a 2 mile 100,000:1 CD ROM map of my
  neighborhood.  Zoom in to 3909 07636 and see his work.  He will do these
  maps for you, but please recognize it takes 4 to 6 hours each, and  you
  should make a sizable contribution ($45?) to his WIDE Digi fund! hi hi

Ver 71c&d: more tweaks for SAREX:
* Fixed SPACE mode to better predict oerhead passes (95 mins vice 91)
* CONTROLS-FILTERS-GRID mode will decode a GridSquare in the TO callsign
  of a packet.  Good for shortest possible posit report (for Meteor Scatter)
* Packets with CZAR will show red
* Map borders now keep up with out-zooming
* Hook on PLIST now UPlink command toggles on/off vice QUIT/UPLINK
* Changed CONTROLS-FILTERS-GATE to HFgate

Ver 71b: More tweaks:
* From NOW ON, only WIDE-RELAY digipeaters will be shown as GREEN
* Better SPACE mode.   See Space.txt
* Added  $PGRMA for Garmin altitude
* Added QRT mode (F6) which forces your SPEED to ZERO as you approach any
  destination.  This keeps others from DEAD RECKONING you forever...

Ver 71a:  Took my first Doppler DF fox hunt with APRS, 
and really had fun!  See new DF.txt.  Lessons learned:
* Replay DOPPLER.hst to see our track.
* Fixed INPUT-SAVE and INPUT-UP which didn't work in 71
* Fixed BULLETIN display format that got broken in 71
* New INPUT-HEADING cmd for entering a COMPASS heading when stopped with GPS
* Neither Manual RELATIVE bearings nor automatic DF bearings are accepted
  if the vehicles current HEADING is 000 or does not exist
* If Validated for DF and GPS NMEA speed drops below 4 knots, then Heading
  is NOT UPDATED.  Last CSE is still used.
* Pings are no longer trapped on L-list
* Tried to remove cmd:cmd: glitches

Ver 7.1:  Major changes to MAP distribution.  I have been adding most of
the roads from 64 mile maps into the larger regional maps such as ARLAMSAL,
IAILINMO, TXstate, OH-MI-WV and CAlif.  This allows me to move these 64 mile 
maps to the regional distro map zips instead of all of them being in the 
basic USA distro.  This makes the basic APRSxx.zip file smaller and the 
regional Xmapsxx.zip files larger.  This trend will continue.  This process
requires balancing all of the MAPLIST.USA, EAS, CEN, WES and SE, so please
report any errors, omissions or heirarchy problems.  To see my
boundaries between regional distributions go to USA map and hit MAPS-ALT
comand.  The Ohio mapmaker extrordinare, KB8JXO, has done over 90 maps of
Ohio and is now spilling over into other states.  He will make you a map
for a contribution to his WIDE repeater fund...  Estimate 4 to 6 hours labor
per map...
* Fixed DF code so dual port DF and TNC/HSP modes both work at same time
* Added DF Single Port mode so TNC, GPS, DF can all share one comm port!
* Added F8 key to force an instant HSP/GPS fix.
* Added INPUT-SAVE-my command to mark, and save your present posit as an OBJ
* Added INPUT-UPLINK-my.  Same as above but also uplinks the OBJ.
  These commands are useful for marking a DF fix on the map while you continue
  to drive to a new location.  See DF.txt.
* Added the ability to specify a special OPS-DIGI path for each outgoing
  message.  This has advantages and drawbacks.  See Help.txt

Ver 7.c:  Improved Chess game with better symbols, and Alt-S-OTHER-GAME mode
See end of new README\APRS.DOC.
* Added alt-S-MODES-altNET command to permit operation of a subnet on an APRS
  freq without cluttering up everyone else.  This is the converse of IGNORE
  mode.  See details in HELP.TXT under alt-S SETUP descriptions
* Added alt-S-GPS-NMEAlog command for toggling on a log of NMEA data

Ver 7.b:  Fixes bug in 7a dealing with #1 map HOT key.  Also adds MASS maps
* Adds SPACE mode (same as Grid-Sq mode but it BEEPS if U are successfull!)

Ver 7.a:  Upgraded to MAPFIX12 that can now KILL Labels, making it easier to
get all the map labels in the right place.
* 7.0 stations receiving a message QUERY vice the new OPS-QUERY would not
  ack the query resulting in no message movement on the sender until that
  ?APRS? message was erased.  Now, 7.a does ack a message Query, for backward
  compatibility, but using the new OPS-QUERY-Callsign, is preferred.
* MAPS-PLOTS-RANGErings now plots in Great Circle Range and Bearing
  Above 1024 miles an additional yellow line shows the actual Bearing
* APRS now supports ARNAV data formats in SPM/HSP modes (for aviation GPS's)
* GATEWAY filter to ignore packets via GATE. (CONTROLS-FILTERS-GATE)
* Can select Kilometers vice statute miles for Range (CONTROLS-Km)
* APRS now handles ECHO/WIDE aliases for KAM when band switching
* KN4IM suggests trying 14.105 keyboarding freq for 20M APRS.  Although APRS
  is not as effecient as a CONNECTION for keyboarding, it is an IDEAL tool
  for monitoring a Keyboard channel.  Also the 14.100 LSB we had suggested
  gets a lot of QRM from the 14.099 BBS freq.


Ver 7.0:  Two changes that are NOT backward compatible.  1)  To accomodate
NWS watch boxes up to 400 miles long, the APRS OBJS-AREAS-LINES shapes are
now 4 times bigger.  All stations in a network using these symbols must 
upgrade to 7.0.  2) MAPFIX1.bas now has an optional compression feature.  
If maps are compressed (60% size and 33% speed) then only 7.0 can use them.
Save all original maps as xxxx.ORG so that you can always go back to the 
original for such commands as the IMPORT and OVERLAY.  Since they are already
somewhat compressed, there is NO advantage in compressing them before
zipping them for distribution.  The main advantage of compressing a map is 
on a slow 8088 laptop running from a floppy.  I suggest that all maps should
remain uncompressed except by an individual for his own use.
Other changes:
# New 32 mile maps from 2,000,000 CD ROM is EASY using MAKEMAPS1.bas/exe!
  If you have the CD, start cranking them out..  Here are some new ones:
  GA-ATL, WAsound, WAsoundN, Better Florida/Caribean overlaps
  RINewprt, ARLAMSAL, GAnwest, MTBoz-ne, ORnwest, WYellow(stone)
# With this new speed of making 32 mile maps, I am further splitting disto
  versions to EAST, SEAST, WEST, CENTRAL, MIDWEST.  See MAPS.txt or use
  MAPS-ALT command on the USA map to see the regions
# Eliminated NC-SC-GA.map which is all included in USASEAST
# Moved many 64 mile maps from standard distro into regional distro
# Improvement to MAKEMAP1.bas/exe to use a more optimum scale to help reduce 
  the grainyness of 30 mile maps from the 1:2,000,000 CD ROM.
# New MAPFIX1.bas/exe has OVERLAY command to temporarily overlay or
  compare maps.  Also has new compression technique.  Useful for laptops.
# Have defined color 2 (light green) to represent ADMIN Boundaries (Parks)
# New-feature HotKeys for instant beginning of each new digitizer line
# New MAKEMAP1.bas/exe now reduces the number of points generated in
  Boundaries, Streams, and railroads compared to Roads.
* Force load of BACKUP file by invoking APRSxx/B
* Replay raw NMEA GGA and RMC files if file ends in .DOS
* Fixed crash on too-far zoom for DF stations and for OBJ-AREAS...
* Will now accept $PGRMZ (Grmn) and $PMGLB (Mgln) Altitude formats
* Fixed quirks in saving DIGIPEATER table
* Force 0000 posit for GPS configured start-up so your HOME posit is NOT xmtd
* MAPS-BORDERS display now ONLY draws one size of borders at a time
* Changed OBJ-AREAS-LINES to permit 400 mile shapes (WX WATCH BOXES). THIS
  IS NOT BACKWARDS COMPATIBLE.  EVERYONE in a WX net MUST upgrade..
* Added GATEWAY filter to filter out all posits beyond a given range
* Changed CONTROLS menu to make room for GATEWAY filter
* added JUNK filtr to NOT print lines with ctrl chars to save map fm scrolling
* Fixed XMT-PACKETS command to prevent permanent 8 sec lockout at midnight
* Query-one-station is no longer treated like a message, but is initiated
  with the OPS-QUERY command.
* New TROUBLE.TXT has some trouble shooting hints

Ver 69:  Fixed the major bug that ignored ALL FUTURE GGA's once a single
bad NMEA was received!  This bug has probably been in there since 68a.
* Better compile saved 32K!  EXE is now 345K vice 377K
* Added Admin boundaries, Cultural Features and Railroads to MAKEMAPS
* Vy minor tweak to MAPFIX68 to default to existing origin on F2-CONVERT
* 8 New Florida maps in FLmaps01.zip
* DX mode sorts DX messages on the DList.

Ver 68e: Found out that 68c & d may crash on GPS modes due to the post-dayton
fix which does NOT first draw a map for mobiles.  This causes a crash when
the first fix comes in and tries to plot it on a non-existant map! ARGH!

Ver 68d: Found MAJOR flaw in maps generated by MAKEMAPS.bas. Fixed it and
maps and released 68d as well: (STUPID IDEA!)
* Fixed MAPFIX68 so that it replays GPS Tk Hsts in S. and E. Hemispheres
* Added NCobanks and 3 SC maps to SEMAPS
* Better MAC smbol
* Better F9 will NOT use WORLD map if Calif and NewEng stations are on
* Better program ABORT if NO Maps or MAPLIST or MAPS directory
* Fixed 100ths rain readings at top of screen

Ver 68c: Lessons learned at Dayton while driving with floppy CGA laptop!
* Boots to Plist vice MAP in GPS modes
* Fix so CGA's do NOT crash, but ignore F7 switch to 43 line mode.
* NO auto-switching to READ scrn on CGA's due to SLOW map-redraw requirement
* MAPS-WHICH command 
* alt-SETUP-GPS-NOgps can be toggled on/off without needing to re-validate
* Added Jet and Police to menu
* NWS watch/warning box to OBJ-AREAS (x miles either side of a line)
* Killed OBJ's fade to gray
* Default MAPLIST.USA, vice .APR.  Use CHG-MAPlst command
* Removed DF validation prompt unless you are DF configured.
* Automatic HF/VHF switching for PK-232 (un tested)
* SETUP-OTHER-AGL sets average Gnd level so Mobiles do not FLY in 3D
* increased WX alarms to 999 
* Added 2port KAM Xmission.  
* Fixed CONNECT=> BLUE COMM SCREEN
* Added ARNAV experimentally in the SPM mode. Needs test?
* MAP-LOCK no longer tries to load WORLD
* Fixed F9 which had been ignoring calif
* NEW MAKEMAPS.bas simplifies making 2,000,000:1 maps. See CDROM.txt

Version 6.8b:
* DX MODE had bug since 67 because DXcalls.DAT was moved to SYSTEM dir
* CONV100C.bas by W7KKE no longer crashes on city streets
* Added NWS symbol for N4BYU
* MAX beacon period upped fm 12 to 40 mins if unmanned
* Improved MAC symbol
* Eliminated Dupes of max-length lines on Traffic display.
* APRS now warns LID's using DIGIS on HF
* Telemetry page refreshes in real time and displays in LAST first order

Version 6.8a: Fixed occassional VTG crashes and /raw* bug.
* FROM callsign on BLTN and TRAFFIC pages to full length
* Changed on-air RAIN format to Rxxx in hundredths or Rxx in 10ths

Version 6.8: Fixed bug that prevented GPS RMC sentences from working on OWN
station in both dual-port and HSP mode!  New COMPILE chopped off 30K 
* Select GGA-only in alt-SETUP-GPS to force altitude
* KAMs dont get GATE-BITCH note while operating VHF 
* SEPARATE screen for MSGS
* Swapped R and T commands.  
* DX Cluster is now under alt-SETUP-MODES
* Fixed 3D altitude display in 43 line mode
* RESTORE.TNC is now in APRS\SYSTEM Directory.
* Fixed 128 mile range round off error
* OPS-DIGI is more user friendly
* OPS-UNPROTO avoids the MAP scroll on entering long paths

Version 6.7b: More tweaks:
* Added SLAVE mode so that multiple APRS PC's can all be connected to the
  same TNC via DIODE-OR circuit.  This allows all OPERATORS at an EOC
  to have their OWN APRS display, but only need one radio /TNC.  See OPS.txt
* Split out SOUTHEAST maps into SEmaps01.zip
* Fixed MAPFIXER again.
* Restored OBJECT AREAS, boxes, triangles, circles which got lost somewhere
* Initializes from InitTAPR.TNC or InitAEA.TNC
* Added OHbooths.map
* U-II WX reports are no longer always saved in HIST 

Version 6.7a: Minor tweaks 
* Unique BEEP when someone PINGS.
* Added selective prompt to Xmt command 
* Changed FILE-REPLAY to NOT always re-draw the map
* Fixed Alt display so CALLS do not overwrite Alt scale

Version 6.7:  Squished out 18k, but filled it back up:
* Added 3D display of Aircraft and Balloons. 
* New altitude format:  /Axxxxxx  (6 digits)
* Combined CAP.txt into AIRCRAFT.txt.  Combined README.100 into CDROM.txt.
* New SYSTEMS subdirectory (Now REQUIRED!)
* Abort any MAP while drawing by hitting any KEY.
* Fixed some probs in MAPFIXER and RENAMED to MAPFIX67.bas(still screwed up)
* RE-named MISSOURI,TEXAS,ALASKA,ARIZONA,VIRGINIA maps to XXstate.map


Version 6.6:  Added MOUSE cursor, HOOK and ZOOM capability to both MAP
and P/L-lists.  Also use mouse in MAPFIXER to move cursor and add points.
Also in MAPFIXER, you can use the MOUSE as a POOR-MANS-DIGITIZER!
See MOUSE.txt

Version 6.5c:  HSP was in-op in 6.5 and later. Fixed it.
* "Toggling NMEA..." will show "Got good NMEA..." if successful.
* Can Kill a HOOKED object on map screen
* Changed DF and POWER plots to OVERLAY the map

Version 6.5b:  OOPS
* Fixed bug that prevented WIDE digi's from showing up green

Version 6.5a: TOTAL reorganization of DISTRO disk.
* See MOREMAPS.txt for changes to MAP distro
* MAPLIST.xxx extension now shown on CONTROLS display
* Fixed BUG with GPS ssid-7 crashing on headings less than 10 degrees
* Added SLOW/MED to REPLAY 
* Fixed DEW point
* Fixed STREETS interface to include passing SSID on calls
* BEEPSoff includes MSG beeps
* 30 % better MAP drawing times 
* JUST now does MOBILES, WEATHER, and LATEST


Version 6.5: Major internal changes to make more room. Look for minor bugs.
* MAJOR NEW TELEMETRY FUNCTION!  Added MILEPOST function.  See TELEMTRY.TXT.
* high-res text on maps and other screens
* Instant video page switching so MAP does not have to be re-drawn!
* Nag box for HF'ers that use ECHO
* More SETUP menus
* Fades old CALLS as well as the symbols

Version 6.4b:  Changes QUERY Latitude to (-) in W Hemesphere effective 1 Apr.
Changes small triangle from (c) to (n).

Version 6.4a: OOPS, 63c and 64 would NOT let you change WX
alarms nor configure a second COM port for GPS/WX/DF.

Version 6.4:   Changed PROMPTS to YELLOW, Warnings to RED etc
* Wrote SUMMARIZ.bas to scan BK and HST files to produce a SINGLE ALLPOS.hst

Version 6.3c: Removed query on start-up for registered users to reduce QRM
* Much improved VIEW screen
* Still better OPS-FIND displays
* SMALLER SYMBOLS! 
* User defined SSID defaults for special nets.

Version 6.3b: APRS TELEMETRY announcement!  
* Fixes 63a bug that dropped AutoQuery on start-up.

Version 6.3a:
* FIxes bug that prevented reloading TRAFFIC from BACKUP file
* Better display of DIGIS on hooked display
* Accepts commas in manual WX reports
* Implements QUERY at a RANGE
* Adds WX ALARM RANGE

Version 6.3: Same as 62d but adds WD8QWR & W1TTY suggestion for COM3,4  
I POKE BIOS to think that COM3=1 and COM4=2.
* OPS-FIND automatically hooks on P and L lists.

Version 6.2d:  Minor changes
* Fixed DIGI-path display when hooked
* Finished all 15 default SSID symbols
* Fixed ACK message problem on short msgs
* Displays all RAW stand-alone-trackers in light gray
* Disables auto-logging for NEW users
* Save WIDE alias in config file
* OPS-FIND now asks before re-drawing map off screen


Version 6.2b:  1) Latest Magelan Meridians have dropped the RMC sentence.
* MAPFIX renamed to MAPFIXER and uses high-res text
* Rain Alarm in 10ths.  * All alarms defaulted to MAX
* Enter WIND in KPH and Temp in Celcius (still xmitted as MPH & F)
* Page back to page 1
* DIGI list shows direct*
* SCREEN.txt describes APRS screen
V 6.2a fix to rain alarms that culdnt be turned off in 6.2!
* BEEPS turns off the un-registered-user-page-full beeps.

VERSION 6.2: Fixed too sensitive WX alarms!  Added better checking of 
POSITS.  New ideas in HF.txt, and AIRCRAFT.txt.

VERSION 6.1:
* FRQCOORD.txt on using APRS as a FREQ-COORDINATION tool
* 70Chanls.2M on finding SEVENTY 9600 baud channels on 2M !!
* WX alarms when WX thresholds are exceeded
* Considering a remote DIAL-IN modem mode
* N2IPH wrote APRSMICE.txt on interfacing a MOUSE to APRS!


VERSION 6.03  Sent raw CD ROM data to to Iowa, Minnesota, and Missouri.
* Upped points to 3600 (later reduced to 2999) and active maps to 170
* Old posits painted blue
* Fixed DATE-TIME stamp on OBJects that was defaulting to 000000
* TRIM and IMPORT commands in MAPFIX now leave no garbage
* 100toGRF.bas 

VERSION 6.02  Added an AMTOR/PACTOR mode.  TNCinit now also sets NEWmode 
OFF so that if someone connects to you, your TNC
will NOT get stuck in COMMAND mode.  Added SSID defaults for ARNAV.

VERSION 6.01  Lessons learned from Marine Corps Marathon 94.
* INPUT-MY fixed to use current time, vice old time
* Added ARNAV interface
* Send msg to LOG puts a log entry in the LOG file
* Upped active maps to 160 and points to 2000
* Began removing small maps from distro.
* REJect msgs now continue transmitting

VERSION 6.0Plus+ (No changes to 6.0 EXE)
* ALL-ROM DIGIPEATER ideas in IDEAS.TXT
* UHF-FREQ.txt 
* MAPFIX can IMPORT roads from other maps

VERSION 6.0:
* Renamed all README files. Now available F1(HELP)-FILES.
* Alt-IGNORE command sets UNPROTO path to SPCL.
* DF reports now sent at the POSRATE period, only when there is DF data;
* Changing WX values reset the Period to POSRATE.
* Wind above WIND THRESHOLD resets Period to POSRATE.
* Suggested mod N7LUE DF to accept TNC PTT to disable DF during PTT
* NJnorth, NYcityLI & better map switching there
* Plist shows RAW NMEA from stand-alone-trackers
* Wrote MOTOROLA.BAS for sending NMEA commands to M. OEM GPS card with ck-sum
* Solved DXspots w/o Gridsquares sometimes showing up as GridSquares
* OPS-FIND now HIGHLIGHTs calls
* Added Circle/Box/etc AREAS as objects.

VERSION 5.9c:
* Added CONTROLS-FADE
* Fixed MAPS-PLOTS-DF so that ALL null-reports were plotted.
* Space bar re-draws during REPLAYS

VERSION 5.9:  Lots of problems with 5.8.
* 5.8e Alternate MAPLIST.xxx can be reloaded from config file
* 5.9  Fixed INPUT-ADDS for uplinks
* 5.9  Fixed KILL function
* 5.9  MAP-HIERARCHY!
* 5.8L A one-time mod for LORANs mentioned in Aug 73 Mag for $25

VERSION 5.8d:  Added FADE-CIRCLE technique.
* DF in Magnetic if the MagVar is set in SETUP
* ERASE BULLETINS
* FILES-ChgMapLst
* SEND preloads HOOKED call
* MAP-OVERLAY.
* Better protection from on-air garbage
* VIEW buffers last 20 packets.
* Added DIGIpath to hooked display
* Added VORTAC symbol.  See Alaska below 128 mi.


VERSION 5.8c:  5.8c fixed 5.8b bug with U-II that prevented Track
histories from saving, and caused excessive LOGS.  5.8a improved
REMOTE-U-II.  5.8 was General cleanup of code.  New .BK format
* Better CONTROLS/SETUP including VIA and MYalias
* Easier DF inputs for objs and own station
* Better BULLETIN processing by sender
* Added channel capacity
* Increased A/D/L pages to 5
* Upped DXCC calls list to 450 by W8RIK
* CW speed & Test mode.  Full DXcalls sent, and optionally freq.
* Added HEARD to hooked disp
* OBJects no longer on L-List
* LAT/LONG prompts pre-loaded with cursor
* Airplane shows heading
* APRS warning for no digipeat
* AUTOWX prgm by N5KOA for using PCxt for stand alone WX
* Added interface to STREETS-ON-DISK.

VERSION 5.7c:
* Save different DIGIpaths
* Fixed the OPS-COMM-GPS(HSP)
* AUTOTRACK mode to replays
* OPS-FIND
* Overlaying CAP grids on replays
* Fixed DF bug with 0 heights!
* Fixed #5 crash on DX shared freqs

VERSION DF01 and 02:  Beta tests of OMNI-SIGNALSTRENGTH DF routines

VERSION  5.7:
* Fixes LOCAL/ZULU probs during DR
* MAP-LOCK
* Added MyPOS to INPUT command
* MAP-PWR plots!
* Modified COMM-GPS, to see GPS in HSP mode.
* Save BText in CFIG file
* Fixed SHELL bug on CGA
* NoGPS mode to turn off SPM or HSP
* Squelches BEEPS on BULLETINS.
* ZULU fixes to become effective 1 Nov 1994.

5.06:  Added APRS BULLETINs. Improved scrolling on ALL in DX cluster mode.
* SHOW now zooms map to appropriate size
* Added freq to DF prompts
* BText saved in config file

5.05:  DX Clusters MODE!
* DX MAIL lists to the D-List. * DX ANNOUNCEMENTS to the ALL-LIST
* TALKS in the READ-MAIL list. * Better GS plotting
* Upped DXCALLS.dat to 350.    * DX spot prefixes in CW
* 505c fixed L-list bug ignoring normal BEACON texts
* 505d Initializes AEA TNC's to MON 2
* 505e Added plotting of SHOW/STATION and WWV/WX spots
* Added New Orleans for CAP convention

5.04:  Fixed bug that caused all new objs after 1st to be deleted!
Added HELO symbol and BALLOON3.hst

5.03a:  Fixed DSI Doppler DF interface. Added symbols to maps.
Doubled ACK's on dupe lines.  Added more VEHICLES,etc.  Added 
THOMAS MAP grids to SanMateo area.

COMMERCIAL VERSIONs TO OTHER SOFTWARE PACKAGES: See COMMERCL.txt.

5.03:  Added 10 lettered symbols.
* Fixed double-transmit on T key. Added JUST-LATEST command.

5.02:  Consumation of 501a,b,c new MENU wrinkles
* 10 new numbered Balls. F9 centering Key. More symbols & SSID defaults
* GOTO command. * TAB shows CONTROLS and SETUP
* Suppressed 25th line during HSP/GPS. Fixed RMC prob with no
  course and speed! TRAFFIC & READ-MAIL saved in BACKUP.
* RAIN reports /Rxx per hour and /Pxx per day
* Fixed delayed-MYCall for CAP, etc
* Display raw GGA data on 25th line

5.00 ALL NEW Menu commands. Realtime Overwrite of P-LIST. Latch on View page.
     GPS-time sync. Map hot keys. Parse raw U-II data. New Balloon/Bikes. New
     DSI DF interface. SE ID, NW FL, NE FL maps. Fixed null field GPS parsing
405b Fixed KPH/MPH bug.  DAYTON 94 version.
405a Fixed major KILL bug. Forever OBJECTS!  Lots of re-writes for more room!
4.05 CAP grids.  Improved MIR mode makes BCNS/POSITS grid repts identical
     Made U-II and Manual RAIN consistent at .01 inch.


