Capital letters in commands must be entered, others are optional.
Parameters in brackets <> are optional, Parameters separated
by | can be entered alternatively.

 //Access              : User access string (Permissions)
 //Bell                : Call Sysop, maximizes the connect window
 //BInary <on|off>     : auto UUDECODE mode
 //CAp <Filename|off>  : Capture connection to "Filename" (textmode)
 //CD <Verzeichnis>    : Changes home directory
 //Connect P:C:STATION : Connect "Station" E.g."//C 0:1:OE8XPR-2"
 //Del File            : Deletes "file" (wildcards allowed)
 //Dir <Filter>        : List directory  E.g "//D *.txt"
 //Echo text           : Sends string "text" back to you
 //ESc                 : Stops a running file transfer (//GET)
 //Exit                : Disconnects and closes Pr4Win
 //Get TextFile        : Sends File "TextFile" in textmode (wildcards allowed)
 //GB BinaryFile       : Sends File "BinaryFile" in #BIN# mode. (wildcards allowed)
 //GU BinaryFile       : Sends File "BinaryFile" UUENCODED (wildcards allowed)
 //Help <?|Command>    : Sends this helpfile or help on "command"
 //Info                : Sends station info ( CNF\INFO.TXT if exists)
 //Last                : Sends date and time of last connection
 //Mail <Title>        : Leave a message for the sysop
 //Min                 : Minimizes the connect window
 //MOnitor             : Sends a List of heard callsigns (last 20)
 //Name <Name>         : Enter your name
 //PAr                 : Shows AX25 and TRX Parameters
 //PLay <?|Sound>      : Play a sound, ? shows sounds in cuurent dir
 //POrts               : Shows Pr4Win devices (COM and TCP/IP)
 //PRompt <on|off>     : Switches Prompt on or off
 //PSD                 : Shows save directory
 //PWD                 : Shows home directory
 //Quit                : Ends a Connection
 //QTh <Qth>           : Enter your QTH
 //Rem Remark          : Enter "remark" into the logbook
 //Run Program         : Starts program
 //RX file             : Starts wating for file with XMODEM protocol 
 //SCD Path            : Changes save path
 //SDel File           : Deletes "file" from save directory E.G."//SDel *.txt"
 //SDir <Filter>       : List save directory  E.G "//SDir *.txt"
 //SErver <service>    : Shows available servers, connects a server
 //Statistics          : Show Frame-statistics
 //SX file             : Sends file with XMODEM protocol
 //Version             : Show Pr4Win Version

Enter each command at the beginning of a new line and
terminate each command with CR.

All remote commands can be invoked locally by entering a "!" as a first
letter followed by the remote command. E.G. "!//INFO" sends your info
file to the connected station.

You can get more detailed information on each command using
the "//HELP COMMAND" command.
